|  |  |
| --- | --- |
|  | **Government College of Engineering, Jalgaon,Government College of Engineering, Jalgaon National Highway No-06, Jalgaon- 425002.** |

**INVITATION LETTER**

|  |  |
| --- | --- |
| **Package Code: TEQIP-III/2019/MH/coej/108** | **Current Date: 18-Jul-2019** |
| **Package Name: GCOEJ\_CE05 Rev** | **Method: Shopping Goods** |

To,

**Notice Board**

**Government College of Engineering, Jalgaon**

**Sub: INVITATION LETTER FOR GCOEJ\_CE05 Rev**

Dear Sir,

|  |  |
| --- | --- |
| **1.** | You are invited to submit your most competitive quotation for the following goods with item wise detailed specifications given at Annexure I, |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No** | **Item Name** | **Quantity** | **Place of Delivery** | **Installation Requirement (if any)** |
| 1 | Plate Bearing Test App. | 1 | Govt. College of Engineering, Jalgaon, 425002 | Training and installation for 2 days with company cost. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **2.** | | Government of India has received a credit from the International Development Association (IDA) towards the cost of the **Technical Education Quality Improvement Programme [TEQIP]-Phase III** Project and intends to apply part of the proceeds of this credit to eligible payments under the contract for which this invitation for quotations is issued. | | | |
| **3.** | | **Quotation** | | | |
|  | | 3.1 | | | The contract shall be for the full quantity as described above. |
|  | | 3.2 | | | Corrections, if any, shall be made by crossing out, initialling, dating and re writing. |
|  | | 3.3 | | | All duties and other levies payable by the supplier under the contract shall be included in the unit Price. |
|  | | 3.4 | | | Applicable taxes shall be quoted separately for all items. |
|  | | 3.5 | | | The prices quoted by the bidder shall be fixed for the duration of the contract and shall not be subject to adjustment on any account. |
|  | | 3.6 | | | The Prices should be quoted in Indian Rupees only. |
| **4.** | | Each bidder shall submit only one quotation. | | | |
| **5.** | | Quotation shall remain valid for a period not less than **55**days after the last date of quotation submission. | | | |
| **6.** | | Evaluation of Quotations: The Purchaser will evaluate and compare the quotations determined to be Substantially responsive i.e. which | | | |
|  | | 6.1 | | are properly signed; and | |
|  | | 6.2 | | Confirm to the terms and conditions, and specifications. | |
| **7.** | | The Quotations would be evaluated for all items together. | | | |
| **8.** | | Award of contract The Purchaser will award the contract to the bidder whose quotation has been determined to be substantially responsive and who has offered the lowest evaluated quotation price. | | | |
|  | | 8.1 | | Notwithstanding the above, the Purchaser reserves the right to accept or reject any quotations and to cancel the bidding process and reject all quotations at any time prior to the award of Contract. | |
|  | | 8.2 | | The bidder whose bid is accepted will be notified of the award of contract by the Purchaser prior to expiration of the quotation validity period. The terms of the accepted offer shall be Incorporated in the purchase order. | |
| **9.** | | Payment shall be made in Indian Rupees as follows: | | | |
|  |  |  | **Satisfactory Delivery & Installation - 10% of total cost Satisfactory Acceptance - 90% of total cost** | | |
| **10.** | | | Liquidated Damages will be applied as per the below:  Liquidated Damages Per Day Min % :N/A  Liquidated Damages Max % : N/A | | |  |
| **11.** | | | All supplied items are under warranty of **12** months from the date of successful acceptance of items and AMC/Others is **.** | | |  |
| **12.** | | | You are requested to provide your offer latest by **05:30** hours on **01-Aug-2019.** | | |  |
| **13.** | | | Detailed specifications of the items are at Annexure I. | | |
| **14.** | | | Training Clause (if any) **Training and installation for 2 days with company cost.** | | |
| **15.** | | | Testing/Installation Clause (if any) **Training and installation for 2 days with company cost.** | | |
| **16.** | | | Performance Security shall be applicable**: 0%** | | |
| **17.** | | | Information brochures/ Product catalogue, if any must be accompanied with the quotation clearly indicating the model quoted for. | | |
| **18.** | | | Sealed quotation to be submitted/ delivered at the address mentioned below, **Government College of Engineering, Jalgaon,Government College of Engineering, Jalgaon National Highway No-06, Jalgaon- 425002.** | | |
|  | **19.** | We look forward to receiving your quotation and thank you for your interest in this project. | | | |

(Authorized Signatory)

Name & Designation

**Annexure I**

|  |  |  |
| --- | --- | --- |
| **Sr. No** | **Item Name** | **Specifications** |
| 1 | Plate Bearing Test App. | The Plate Bearing Test is essentially a model test of foundations. It gives the load deformation characteristics for determining the ultimate bearing capacity of foundations. This test is a standard technique for determining bearing capacity of soils and the results of other methods are compared and calibrated with the values obtained with plate bearing test. In this method, a steel plates is subjected to a gradual increment of load and the corrosponding settlement is noted. The Ultimate Bearing Capacity is taken as the load at which the settlement increases at a rapid rate. Plate Bearing Test Apparatus Ref. standard IS: 1888 The equipment consist of the following replaceable parts:  i) Hand Operated Hydraulic Jack, Capacity 500kN (50,000 kgf) 1 No.  ii) Hydraulic Hand Operated Pump with 200mm Dia. Load Gauge Capacity 500 kN (50,000kgf) High Pressure flexible metal Pipe 5 Meter long. 1 No.  iii) Ball and Socket Arrangment Cosisting of two steel plates, with one steel ball in-between the plates 1 No.  iv) Extension Rod long, 12mm dia x 25cm for taking Dial Gauge readings. 16 Nos.  v) Magnetic base with female thread on top, for holding extension rod. 4 No. vi) Top End Plate 50 mm dia with male thread, for fitting on to the Extension Rods and positioning the Dial Gauge and Plunger. 4 Nos.  vii) Column 15 cm dia x 25 cm long with flanges, complete with four bolts and nuts. 2 Nos.  viii) Column 15 cm dia x 50cm long, with flanges, complete with four bolts and nuts. 1 No.  ix) Datum Bar light weight, portable, total span 5m height approx. 30cm, mounted on two removable legs. (It is made in two parts. Provision exists for Datum Bar of 2.5m span to be used. A spare leg is provided for the purpose. Complete with two quick release clamps for positioning and holding the dial gauge brackets). 2 Nos.  x) Anchor Spikes 10 Nos.  xi) Quick Release Clamp for positioning dial gauge bracket xii) Dial Gauge 25mm travel, 0.01mm least count 4 Nos.  xiii) Grooved MS Plate 30 cm x 30 cm square x 25 mm thick 1 Nos.  xiv) Grooved MS Plate 45 cm x 45 cm square x 25 mm thick 1 Nos.  xv) Grooved MS Plate 60 cm x 60 cm square x 25 mm thick 1 Nos.  xvi) Grooved M.S. Plate 75cmx75cmx25mm thick 1Nos.  xvii) Load Truss: 200kN Two halves with joist to be bolted together along with anchorage of semicylindrical piece 8 Nos Held by 1m long steel spikes, (102 Spikes) cross pieces are mooved to the anchorages by channel straps ( 8 Nos) and bolts with nuts(16 Nos), guy wires with turn buckets to errect truss. Anchor Straps(8 Nos), guy wire with sixteen buckets-(6 Nos)  Top flange spice plate(1 No) with 8 bolts and nuts, Bolts with nut for bottom spice plate(6 Nos) , sledge Hammer, spanners(2 Nos) |

**FORMAT FOR QUOTATION SUBMISSION**

(In letterhead of the supplier with seal)

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_

To:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Sl. No. | Description of goods \ (with full Specifications) | Qty. | Unit | Quoted Unit rate in Rs.  (Including Ex-Factory price,  excise duty, packing and forwarding, transportation, insurance, other local costs incidental to delivery and  warranty/ guaranty commitments) | Total Price  (A) | Sales tax and other taxes payable | |
| In % | In figures (B) |
|  |  |  |  |  |  |  |  |
| **Total Cost** | | | | |  |  |  |

Gross Total Cost (A+B): Rs. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

We agree to supply the above goods in accordance with the technical specifications for a total contract price of Rs. ———————— (Amount in figures) (Rupees ————————amount in words) within the period specified in the Invitation for Quotations.

We confirm that the normal commercial warranty/ guarantee of ——————— months shall apply to the offered items and we also confirm to agree with terms and conditions as mentioned in the Invitation Letter.

We hereby certify that we have taken steps to ensure that no person acting for us or on our behalf will engage in bribery.

Signature of Supplier

Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contact No. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_